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How to configure the VALMAR-BO-1 indicator
The VALMAR-BO-1 indicator draws a given number of BreakOut Levels based on either:

1. the range of a specified candle or 

2. the open price of a specified candle

for a specified Period.
The indicator can be used on all time frames.  Some combinations of Period and time frame will however result in many lines on the chart.
In the input tab of the indicator the following parameters can set:

	Name
	Type
	Used for

	Buffer
	Int
	Is the number of points that will be added to the range of  the “Base Candle”.

	Periode
	String
	D for daily, W for weekly and M for month, default is W.

	Base_Candle_Time
	String
	Time of the of the “Base Candle”  in format (24hours) h:m, without leading zero for h and m.  

To specify the Candle 5 minutes past 6.   6:5

	Use_Range
	Boolean
	True: The calculation of the breakout levels is base on the range of the “Base Candle”.
False:  The calculation of the breakout levels is base on the Open price of the “Base Candle” +/- Min_Range.

	Min_Range
	 Int
	If the range of the Base Candle is less then Min_range Min_range value will be used. Min_Range is specified in number of points

	NumLines
	Int
	The Number of Breakout levels (in one direction ) that will be put on the chart. Minimum is 3 and maximum is 10.

	Width
	Int
	Specifies the thickness BreakOut level lines in the chart.


